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Fig. 4. 
Log inactivation of (a) MS2 coliphage (UV doses of 40 and 80 mJ/cm2) and (b) bacteriophage T4 (UV doses of 2 and 7 mJ/cm2) in the trials with humic acid floc particles. The “Control” conditions had no humic acid or coagulant added.
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